**SPECIFICATIONS**

GARVO 3 e 5

Supply and installation of waterproof elastic joint covers for use in combination with PLASTIVO coating or AQUASCUD protective system.

The product must be used for:

* Sealing of joints between small prefabricated elements under positive buoyancy conditions
* Waterproofing construction, contraction, expansion and perimeter joints in screeds (ref. UNI 11944), structural joints are excluded
* Sealing of cracks and casting joints in structures subjected to positive hydrostatic thrust

The material must have the following characteristics:

**Specification and Values**

**Working temperature:** -30°C +90°C

**Resistance to acids and bases:** good

**Elongation at breaking point:** > 60%

**Elongation load:** > 24 N/15 mm

as well as GARVO 3 e 5 Volteco or a product with equal or superior characteristics.

The technical data must be supported by test certification issued by an accredited official laboratory and/or be subjected to quality control according to ISO 9001.

For further details on the individual products and installation specifications, refer to the relevant technical data sheets which can be downloaded in the updated version on the website [www.volteco.com.](http://www.volteco.com/)

EN Specifications n. ED | CP | 01 | 00 | W | 08/25

