SANOFER

Supply and installation of cement-based protective coating specific for protecting reinforcement rods.
The product must be applied with a thickness greater than 200-300 microns.
The product must be used for degraded reinforcement bars in deteriorated concrete.



The material must have the following characteristics:
EC Certification according to EN 1504-7


Specification, Test method and Values

Corrosion protection (UNI EN 15183): Specification fulfilled
Shear adhesion (UNI EN 15184): Specification fulfilled


as well as Sanofer Volteco or a product with equal or superior characteristics.
The technical data must be supported by test certification issued by an accredited official laboratory and/or be subjected to quality control according to ISO 9001.
For further details on the individual products and installation specifications, refer to the relevant technical data sheets which can be downloaded in the updated version on the website www.volteco.com.
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