TRIPLEZERO-T

Supply and application of a ready-to-use, superhydrophobic, non-toxic creamy emulsion which, thanks to its immediate water-repellent action, protects walls subject to water absorption phenomena with a variable consumption from 100 to 400 g/m² depending on the porosity of the substrate



The product must be used as a water-repellent protection layer on porous surfaces such as solid bricks, tuff, stone or rock.
The material must have the following characteristics:


Specification and Values

Appearance: white creamy mixture
Density (+20°C): 0.9 g/m3


as well as Triplezero-T Volteco or a product with equal or superior characteristics.
The technical data must be supported by test certification issued by an accredited official laboratory and/or be subjected to quality control according to ISO 9001.
For further details on the individual products and installation specifications, refer to the relevant technical data sheets which can be downloaded in the updated version on the website www.volteco.com.
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