TRIPLEZERO

Supply and installation of a ready-to-use, superhydrophobic, non-toxic creamy emulsion for both internal and external application with a consumption and yield equal to 10 cc / m per every centimeter of masonry thickness.

The product must be used in porous masonry or made of solid brick and/or stone, rock and tuff to reduce capillary rising damp in the masonry by injection.



The material must have the following characteristics:
WTA Certification


Specification and Values

Appearance: white creamy mixture
Density (+20°C): 0.9 g/m3


as well as Triplezero Volteco or a product with equal or superior characteristics.
The technical data must be supported by test certification issued by an accredited official laboratory and/or be subjected to quality control according to ISO 9001.
For further details on the individual products and installation specifications, refer to the relevant technical data sheets which can be downloaded in the updated version on the website www.volteco.com.
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