VOL-TEC

Supply and installation of expansive profile for hermetic sealing of large movement joints, hydraulic sealing and seismic isolation. It is composed of high damping SBR/Natural rubber with modular elements and compression plates made of PA6 resin.
The profile can be fitted with a pair of strings Ø 10 mm made of hydro-expansive rubber for greater pressure on the contact surfaces.

The product must be used for the hermetic sealing of joints with large movement, where a perfect hydraulic seal is required.
Suitable for structural works in reinforced concrete, carried out in areas at risk of seismic and in the presence of an aquifer as well as VOL-TEC Volteco or products with equal or superior characteristics.

The technical data must be supported by test certification issued by an accredited official laboratory and/or be subjected to quality control according to ISO 9001.
For further details on the individual products and installation specifications, refer to the relevant technical data sheets which can be downloaded in the updated version on the website www.volteco.com.
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